{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Tabelle1","Tabelle2","Tabelle3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Tabelle1","index":0,"n_rows":62,"n_cols":7,"rows_kept":62,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
[]
[]
[null,"Ouvrage:",null,"Descriptif type Serge Ferrari SA, CH-8193 Eglisau"]
[null,null,null,"Façade"]
[null,null,null,"Stamisol FI"]
[]
[]
[null,"Article","Prestation","Quantité:","UM","Prix:","Montant:"]
[]
[]
[null,"01","Lés / écran de façade Stamisol FI / largeur 250 cm"]
[null,null,"Matériau: enduction polyacrylate spéciale sur fibre polyester"]
[null,null,"Perméabilité à la diffusion: sD ~ 0.04 m "]
[null,null,"Résistance aux intempéries et aux UV durant une période de 12 mois avant bardage définitif"]
[null,null,"Teinte: noir"]
[]
[null,null,"En particulier pour façades suspendues, ventilées,"]
[null,null,"à joints fermés, ou légerements ouverts"]
[]
[null,null,"Fabricant: Serge Ferrari SA, CH-8193 Eglisau"]
[null,null,"Téléphone: 0041 (0)44 868 26 26"]
[null,null,"Téléfax: 0041 (0)44 868 27 27"]
[null,null,"e-mail: info@stamoid.ch                   www.stamisol.com"]
[]
[]
[null,"02","Lés / écran Stamisol FI","..................","m²",".....................","......................"]
[null,null,"Livraison et pose selon instructions du fabricant"]
[null,null,"(face traitée à l'extérieur)"]
[]
[null,"03","Suppléments"]
[]
[null,"03.01","Exécution des recouvrements,","..................","m1",".....................","......................"]
[null,null,"étanche au vent, avec Stamcoll N55 en pot ou Stamcoll AS."]
[]
[null,"03.02","Raccordement sur maçonnerie","..................","m1",".....................","......................"]
[null,null,"Exécution avec Stamcoll N55 en pot ou en Stamcoll AS"]
[null,null,"Mise en œuvre selon prescriptions du fabricant"]
[]
[null,"03.03","Raccordement sur fenêtres","..................","m1",".....................","......................"]
[null,null,"Exécution avec Stamcoll N55 en pot ou en Stamcoll AS"]
[null,null,"Mise en œuvre selon prescriptions du fabricant"]
[]
[null,"03.04","Raccordement sur renvois d'eau","..................","m1",".....................","......................"]
[null,null,"Exécution avec Stamcoll N55 en pot ou en Stamcoll AS"]
[null,null,"Mise en œuvre selon prescriptions du fabricant"]
[]
[null,"03.05","Raccordement sur gaines de ventilation","..................","pièces",".....................","......................"]
[null,null,"Avec raccord Stamisol"]
[null,null,"Exécution avec Stamcoll N55 en pot ou en Stamcoll AS"]
[null,null,"Mise en œuvre selon prescriptions du fabricant"]
{"$rows_empty":11}
[null,"Total","Façade",null,null,null,"........................"]

{"sheet":"Tabelle2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Tabelle3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}